**Supplier Verification for Elastic Luggage Straps**

**As a supplier of “elastic luggage straps” you must complete this form and return it to us to verify the products to be supplied meet the requirements of Australia’s Mandatory Safety Standard. These products will not be accepted by us or offered for sale on our websites until you have provided this verification.**

**It is illegal to supply “elastic luggage straps” that do not meet the requirements of Australia’s mandatory standard *–***[*Trade Practices (Consumer Product Safety Standards) Regulations 1979*](http://www.comlaw.gov.au/comlaw/Legislation/LegislativeInstrumentCompilation1.nsf/0/653EE7FFD259E012CA256F7100494EFD/%24file/TraPraConProSafSta1979.pdf)(“**the Mandatory Standard”**).

By completing this form you are verifying that the products identified in this form comply with the Mandatory Standard.

|  |
| --- |
| **What products must comply?** An ‘elastic luggage strap’ is any elastic strap(s) or cord(s) permanently joined:(i) having a hook, buckle or other fastening device at each extremity; and(ii) designed to be used to securing luggage or other objects.**EXCLUDED** - The Mandatory Standard does not apply to elasticised cargo nets or elasticised straps specifically made for the purpose of securing a vehicle jack or toolkit within a vehicle. |

|  |  |
| --- | --- |
| **Supplier:** | Name: |
| Business Registration Number: |
| Address: |
| Contact person: |
| Telephone: |
| Email: |
| **Product:** | Description:  |
| Identifiers: |
| **Authority:** | Name: | Sign: | Date: / / |

**Supplier Verification for Elastic Luggage Straps**

| **Supplier Verification** |  | **Tick if Complies** |
| --- | --- | --- |
| **Complies with Mandatory Standard –** Confirmation that the product complies with the Mandatory Standard. |  | YES □ |
| **Warning label** – A visual inspection of the product has been conducted that confirms the following warning is attached to the strap with exact wording:: NOTE: Elastic luggage straps supplied **before 1 July 2019** can comply with **Option A or Option B**.Elastic luggage straps supplied **after 1 July 2019** must comply with **Option B**. |  |  |
| * + - * + **OPTION A (IF SUPPLIED BEFORE 1 JULY 2019)**

**WARNING:** Avoid eye injury. DO NOT overstretch. ALWAYS keep face and body out of recoil path. DO NOT use when strap has visible signs of wear or damage **OR:****WARNING:** Rebounding hooks cause blindness. Place hooks with care. Keep face and body out of rebound path. DO NOT overstretch. DO NOT use when strap has visible signs of wear or damage. |  | □ YES (and supplied before 1 July 2019)**or**□ COMPLIES WITH OPTION B |
| * + - * + **OPTION B (IF SUPPLIED AFTER 1 JULY 2019)**

**WARNING:** Rebounding hooks cause blindness. Place hooks with care. Keep face and body out of rebound path. DO NOT overstretch. DO NOT use when strap has visible signs of wear or damage. |  | □ YES**or**□ COMPLIES WITH OPTION A (if supplied before 1 July 2019) |
| * + - * + the words are in black lettering on a yellow background;
 |  | YES □ |
| * + - * + the word ‘WARNING’ and the words ‘DO NOT’ in upper case black letters not less than 5 millimetres in height;
 |  | YES □ |
| * + - * + the remaining words are upper and lower case as shown above (upper case letters not less than 5 mm high);
 |  | YES □ |
| * + - * + the warning label is conspicuously displayed and permanently attached to the strap (this means it must not be able to be easily removed or torn by hand. Warning labels made form paper are unacceptable).
 |  | YES □ |