**Supplier Verification for Prams and Strollers**

**As a supplier of prams or strollers you must complete this form and return it to us to verify the products to be supplied meet the requirements of Australia’s Mandatory Safety Standard.** **These products will not be accepted by us or offered for sale on our websites until you have provided this verification.**

**It is illegal to supply prams or strollers that do not meet the requirements of Australia’s mandatory standard *–****AS/NZS 2088:2000 Prams and strollers* as amended by Consumer Protection Notice No. 8 of 2007 (“**the Mandatory Standard”**).

By completing this form you are verifying that the products identified in this form comply with the Mandatory Standard.

|  |
| --- |
| **What products must comply?**  **A “pram”** is a wheeled vehicle with a body of box-like or boat-like shape designed to carry a baby or child weighing up to and including 9 kg, primarily in a fully reclined position.  **A “stroller”** is a wheeled vehicle designed to transport a child in a seated position, and which may also be adjusted to a semi-reclined or fully reclined position.  **Combination prams/strollers** can seat children in upright, semi reclined and fully reclined positions, so they are considered **strollers** under the mandatory standard. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Supplier:** | Name: | | |
| Business Registration Number: | | |
| Address: | | |
| Contact person: | | |
| Telephone: | | |
| Email: | | |
| **Product:** | Description: | | |
| Identifiers: | | |
| **Authority:** | Name: | Sign: | Date: / / |

**Supplier Verification for Prams and Strollers**

| **Supplier Verification** |  | **Tick if Complies** |
| --- | --- | --- |
| **Complies with Mandatory Standard –** Confirmation that the product complies with the Mandatory Standard. |  | □ YES |
| **Test report –** Test report obtained that meets the following requirements: |  | □ YES |
| * + - * + provided by an independent testing facility that has accreditation for AS/NZS 2088:2000 (accredited by NATA or from an overseas accrediting body recognised by NATA) |  | □ YES |
| * + - * + clearly and accurately identifies the exact product to be supplied |  | □ YES |
| * + - * + confirms the product meets all the applicable requirements of the Mandatory Standard |  | □ YES |
| **Identification information** – A visual inspection of the product has been conducted that confirms the following information is permanently and conspicuously marked on the pram / stroller: |  | □ YES |
| * + - * + the registered trade name and address in Australia and New Zealand of either the manufacturer, importer or supplier; and |  | □ YES |
| * + - * + the model name or model number of the pram / stroller |  | □ YES |
| **Tether strap** – there is a tether strap to help carers retain control of prams and strollers and any loop in the tether strap has a perimeter of less than 360 mm. |  | □ YES |
| **Warning on tether strap** – the tether strap is permanently and conspicuously marked with the following warning in characters not less than 2.5 mm high (\*either the term ‘pram’ or ‘stroller’ should be used as appropriate): **WARNING: USE THIS STRAP TO STOP THE PRAM/STROLLER\* ROLLING AWAY** |  | □ YES |

**Supplier Verification for Prams and Strollers**

| **Supplier Verification** |  | **Tick if Complies** |
| --- | --- | --- |
| **Warning on pram / stroller** – the pram / stroller is permanently and conspicuously marked with the following notice in a prominent position in characters not less than 2.5 mm high (\*either the term ‘pram’ or ‘stroller’ should be used as appropriate):  **WARNING:**   * **FOLLOW THE MANUFACTURER’S INSTRUCTIONS** * **PUT ON ALL THE BRAKES WHENEVER YOU PARK THE PRAM/STROLLER\*** * **DO NOT LEAVE CHILDREN UNATTENDED** * **DO NOT CARRY EXTRA CHILDREN OR BAGS ON THIS PRAM/STROLLER\*** * **MAKE SURE CHILDREN ARE CLEAR OF ANY MOVING PARTS IF YOU ADJUST THE PRAM/STROLLER\*, OTHERWISE THEY MAY BE INJURED.** |  | □ YES |
| **Warning on harnesses for strollers** – the stroller must be permanently and conspicuously marked with the following warning in characters not less than 2.5 mm high:  **WARNING: USE THIS HARNESS AT ALL TIMES** |  | □ YES  □ NOT APPLY |
| **Warning on non-reclining strollers** - If a stroller’s backrest is not adjustable to recline to an angle of more than 130° to the horizontal, it must be permanently and conspicuously marked with an additional warning (not less than 2.5 mm high) separated from any other warnings, as follows:  **NOT RECOMMENDED FOR A CHILD UNDER 6 MONTHS OLD** |  | □ YES  □ NOT APPLY |